{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Ark1","Ark2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ark1","index":0,"n_rows":10,"n_cols":25,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Navn","Type","SCOP","Lufttrykk varme m3 per minutt","Lydtrykk dB(A)\nOppvarming","Varmekapasitet ved -25°C kW","COP ved -25°C kW","Varmekapasitet ved -20°C kW","COP ved -20°C kW","Varmekapasitet ved -15°C kW","COP ved -15°C kW","Varmekapasitet ved -10°C kW","COP ved -10°C kW","Varmekapasitet ved -7°C kW","COP ved -7°C kW","Varmekapasitet ved +7°C kW","COP ved +7°C kW","Dimmensjoner innedel","Varmekapsitet Nom min max  kW","COP Nom","Tilført effekt nom. (min.–maks.)","Lydtrykk (utendørsenhet) varme","Kjøleeffekt nom. (min.–maks.)","Elektrostatisk filter","Innedel"]
["Daiken STYLISH","Vegg",5.12,null,"19/24/31/41",3.7,null,4.3,null,4.7,null,4.3,null,"5.2 ved -5",null,6.9,null,null,"3.2 (0.8/6.9)",null,null,49,"3.0/0.7/4.5",null,"FTXTA30"]
["Panasonic veggmodell HZ (kraftig 35varianten)","Vegg",5.0999999999999996,15.6,"18 / 25 / 45",3.6,null,null,2,4.6500000000000004,2.36,null,null,4.75,2.44]
["Panasonic veggmodell HZ25WKE","Vegg",5.2,15.6,"18 / 24 / 45",3.43,2.14,4.03,2.33,4.5999999999999996,2.4700000000000002,null,null,4.75,2.5299999999999998,null,null,"295 x 870 x 230"]
["TOSHIBA DAISEIKAI 9 35","Vegg",5.0999999999999996,"5,3- 12","20 / 25 / 44",2.9,null,null,null,4.5,2.21,null,null,5.5,2.41,7.7,5,"293x851x270","4.0 (0.7 - 7.7)","5,00","800 (170 - 2400)",49,"3500 (900 - 4100)","Ja"]
["MITSUBISHI Kirigamine Furo 4300","Gulv",4.3,"3,9 -9,7","19-25-30-35-41",2.2999999999999998,null,null,"1.60 (-22)",4.3,2.2999999999999998,3.6,2.2999999999999998,null,2.6,"1,0-6,6","4,50","600x750x215","4 (1,0-6,6)"]
["Daiken R32 FVXM35F Standard gulvmodell","Gulv",4.0199999999999996,null,"23/26/32/38",3,null,3.4,null,4,null,4.4000000000000004,2.2999999999999998,"4.8 ved -5 ",2.6,6,null,"600 x 700 x 210","4.0(1.1/6.0)"]
["TOSHIBA GULVMODELL 35","Gulv",4.5999999999999996,"2.66 - 9.8","19 / 24 / 42",{"$nulls":4},4,1.95,null,null,4.3,1.98,5.7,3.91,"600x700x220","4.3 (1.8 - 5.7)","3,91","1100 (350 - 1830)",49,"3500 (1700 - 3700)","Nei"]
["MITSUBISHI KAITEKI 6600","Vegg",5.0999999999999996,"4.0-13.7","19-24-29-36-45",3.1,2,null,null,4,{"$nulls":5},4,null,"307x890x233 ",null,null,null,50,"3.5 (0,8-4,0)","Ja +"]
["Panasonic gulvmodell R32","Gulv",4.5999999999999996,10.1,"19 / 26 / 39",2.85,null,3.3,1.73,3.9,2.15,null,null,4.2,2.33,null,null,"600 x 750 x 207","4,30 (0,85-6,20)",null,"1,06 (0,170- 1,830)",null,null,"Nei"]

{"sheet":"Ark2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}