{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Ark1","Ark2","Ark3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Ark1","index":0,"n_rows":12,"n_cols":12,"rows_kept":12,"merged":[[0,5,0,7]],"flags":["formulas_cached_only"]}
["Ant faser","Spenning","Sikring","max effekt","Ladet energi","Ladetid",null,null,"ladehastighet","Ladestrøm","Ladestrøm"]
[null,"V","A","W","kWh","h",null,"m","kWh/h","A, 1p","A, 3p"]
[]
[1,230,13,2990,{"v":10.8,"d":"10.80"},3,":",39,{"v":2.9589041095890414,"d":"3"},{"v":12.864800476474095,"d":"12.86"},null,"En lader"]
[1,230,32,7360,{"v":10.3,"d":"10.30"},1,":",24,{"v":7.3571428571428585,"d":"7"},{"v":31.98757763975156,"d":"31.99"},null,"To i parallell"]
[3,400,16,11072,{"v":10.2,"d":"10.20"},0,":",53,{"v":11.547169811320755,"d":"12"},{"v":50.205086136177194,"d":"50.21"},{"v":16.735028712059066,"d":"16.74"},"Tre i stjerne"]
[1,230,16,3680,{"v":10.7,"d":"10.70"},2,":",54,{"v":3.689655172413793,"d":"4"},{"v":16.041979010494753,"d":"16.04"},null,"En lader"]
[1,230,32,7360,{"v":10.3,"d":"10.30"},1,":",24,{"v":7.3571428571428585,"d":"7"},{"v":31.98757763975156,"d":"31.99"},null,"To i parallell"]
[3,400,16,11072,{"v":10.2,"d":"10.20"},0,":",53,{"v":11.547169811320755,"d":"12"},{"v":50.205086136177194,"d":"50.21"},{"v":16.735028712059066,"d":"16.74"},"Tre i stjerne"]
[]
[]
["Det er antatt at lasten i 3-fasekonfigurasjon er organisert som tre ladere, hver mellom fase og N-leder"]

{"sheet":"Ark2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Ark3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}