{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Ark1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ark1","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
["Varmepumper","Toshiba Daisekai 9 25","Panasonic HZ25 ","Kaiteki 6600",null,"Toshiba shorai 35","Panasonic NZ ethera 7,2","Panasonic NZ Ethera 6,0"]
["Årsvarmefaktor (SCOP)",5.33,5.2,5.0999999999999996,null,4.5999999999999996,4.5999999999999996,4.5999999999999996]
["Energiklasse","A+++","A+++","A+++",null,"A++","A++","A++"]
[]
["Oppvarming ved 7 °C utetemperatur"]
["Varmeeffekt nom. (min./maks.)","3200 W (700-6700)","3200 W (850-7300)","4000 W(1000-6600)",null,"4200W (1000-7700)","4000 W (850-7200)","3400 W (850-6000)"]
["Tilførteffekt nom. (min./maks.)","600 W (170-1900)","570W (170-2150)","800 (N/A)",null,"950W (200-2330)","909 W (165-2300)","700 W (165-1630)"]
["Effektfaktor nom. (COP)",5.33,5.61,5.0999999999999996,null,4.42,4.4000000000000004,4.8600000000000003]
[]
["Oppvarming ved -7 °C utetemperatur"]
["Varmeeffekt ved maks kapasitet","4400 W","4700W","N/A",null,"4400W","4500 W","3800W"]
["Tilført effekt","1588 W","1926 W","N/A",null,"1774 W","2153 W ","1551 W"]
["Effektfaktor (COP)",2.77,2.44,"N/A",null,2.48,2.09,2.4500000000000002]
[]
["Oppvarming ved -15 °C utetemperatur"]
["Varmeeffekt ved maks kapasitet","3700 W","4500 W","4000W",null,"3000W","4100 W","3200 W"]
["Tilført effekt","1682 W","1898 W",null,null,"1565W","1961 W","1467 W"]
["Effektfaktor (COP)",2.2000000000000002,2.37,null,null,2.2999999999999998,2.09,2.1800000000000002]
[]
["Oppvarming ved -25 °C utetemperatur"]
["Varmeeffekt ved maks kapasitet","N/A","3400W","3100 W",null,null,"2900 W ","2000W"]
["Tilført effekt","N/A","1200 W","1050W",null,null,"1602 W ","1250 W"]
["Effektfaktor (COP)","N/A",2,2,null,null,1.81,1.6]
[]
["Kjøling"]
["Kjøleeffekt nom. (min./maks.)","2500 W (900-3500)","2500 W (850-3000)","3500W (800-4000)",null,"3500W (1100-4500)","3500 W (850-4000)","2500W"]
["Effektfaktor nom. (EER)",5.21,5.43,4.2,null,3.93,4.0599999999999996,4.9000000000000004]
["Energiklasse","A+++","A+++","A+++",null,"A++","A++","A++"]
["Årsvarmefaktor nom. (SEER)",9,7.8,9.4,null,6.3,7.1,7.4]
["Tilført effekt nom. (min./maks.)","480 W (180-800)","460 W (170-670)","820 W",null,"890W (220-1370)","860 W (170-1100)","510 W (170-700)"]
[]
["Dimensjoner"]
["Innedel HxBxD","293x851x270 mm","295x870x230","307x890X233",null,"293x798x230","295x919x194","295x919x194"]
["Utedel HxBxD","630x800x300 mm","622x824x299","550x800x285",null,"550x780x290","622x824x299","622x824x299"]
[]
["Lydtrykk varmedrift"]
["Innedel lav/høy","25/44 db(A)","24/45 dB(A)","24/45 db(A)",null,"27/42 dB(A)","28/42 dB(A)","27/42(A)"]
["Innedel stillemodus","20 db(A)","18 dB(A)","19 db(A)",null,"25 dB(A)","21 dB(A)","19 db(A)"]
["Utedel maks.","47 dB(A) ","47 db(A)","50 db",null,"47 db(A)","48 db(A)","48 db(A)"]
["Sound power (lagt til 2021)","57 db(A)","61 db(A)","Ikke tilgjengelig"]
[]
["Luftutskifting"]
["Luftmengde (m3/min)","12 (720 m3/t - maks)","N/A","4,0-13,7",null,null,"13,4 (804 m3/t maks)","792 m3/t"]
["Årsforbruk varme:",null,"808 kWt",null,null,null,"852 kWt"]