{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Ark1"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Ark1","index":0,"n_rows":10,"n_cols":9,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,4],[1,0,1,2]]}
["Kalkulator for beregning av oppsett av stående kledning"]
["Mål i millimeter",null,null,"Veggmål-underligger (VS)","Overligger+spalte(OS)",null,"Beregning av Spalteåpning"]
["Totalt veggmål",6000,"mm.",{"$f":"SUM(B3-B5)","v":5952},{"$f":"SUM(B4,B6)","v":258},null,"Ønsket overlapp (mm.) på hver side",19]
["Overligger",148,"mm.",null,null,null,"Overligger (mm.)",148]
["Underligger",48,"mm.",null,null,null,"Spalte",{"$f":"SUM(H4-H3*2)","v":110},"mm."]
["Ønsket spalte",{"$f":"H5","v":110},"mm."]
["VS/OS",{"$f":"ROUNDDOWN(D3/E3,0)","v":23},"stk. Underliggere",null,"LES MEG"]
[]
["Underligger+spalte",{"$f":"D3/B7","v":258.78260869565219},"mm.",null,"Her er en kalkulator for beregning av forbruk av bekledning: "]
[{"$nulls":4},"http://kjeldstad-trelast.no/beregning/materialforbruk/#steg5"]